No.1, Innovation Road II, Hsinchu Science-Based Industrial Park, Hsinchu 30077, Taiwan, R.O.C. 
Telephone: +886-3-577-3335	Fax: +886-3-578-2563, +886-3-577-0936
Email: Sales@mti.com.tw	http://www.mti.com.tw

Universal Single Flange LNBF Specification 
Model No. AP8-TW 

RF Input 
Input Frequency Range	Low Band: 10.7 ~ 11.70 GHz
High Band: 11.7 ~ 12.75 GHz

IF Input
Output Frequency Range	Low Band: 950 ~ 1950 MHz
High Band: 1100 ~ 2150MHz
Output Connector Type	75Ω Female Connector
Output VSWR	2.0:1 (Typ.) @ Room Temperature

Local Oscillator
LO. Frequency	Low Band: 9.75 GHz     High Band: 10.6GHz
LO. Frequency Stability	± 1MHz (Max.) @ Room Temperature
LO. Frequency Phase Noise	-55dBc/Hz@ 1KHz (Max.)
-80dBc/Hz@10KHz (Max.) 
-100dBc/Hz@100KHz (Max.) -105dBc/Hz@1MHz (Max.) -110dBc/Hz@10MHz (Max.) 

Conversion Performance @Room Temperature 
Conversion  GAIN	60dB (Max.)
Gain Variation   (P-P)	5dB (Typ.)
Gain Flatness (across any 26 MHz segment)	± 0.5dB (Typ.)
Noise Figure	Low Band: 0.4dB (Typ.)
How Band: 0.4dB (Typ.)
Image Rejection	45dB (Min.)
Cross Polarization	25dB (Typ.)

Power Requirements
DC Current Consumption:	110mA (Typ.)
Operating Voltage -	Vertical: 11.5 ~ 14 Vdc
Horizontal: 16 ~ 19 Vdc
Band Switching	Low Band: 0 Hz
High Band: 22 KHz ± 4KHz

Environmental
Operating Temperature Range	-40¢J~ +60¢J
Storage Temperature Range	-55¢J~ +80¢J